# *B. DRAFT CONTRACT AND SPECIAL CONDITIONS, INCLUDING ANNEXES*

# DRAFT CONTRACT

SUPPLY CONTRACT FOR EUROPEAN

UNION EXTERNAL ACTIONS

No. HR-RS253-3/vehicle

**financed from the general budget of the Union**

**INSTITUT ZA JAVNO ZDRAVLJE VOJVODINE**

**Futoška no. 121, 21000 Novi Sad**

**Registration number: 08246912**

**VAT no. 100452714**

(‘The contracting authority’),

of the one part,

and

<Full official name of contractor>

[<Legal status/title>][[1]](#footnote-1)

[<Official registration number>][[2]](#footnote-2)

<Full official address>

[<VAT number>][[3]](#footnote-3),

(‘the contractor’)

of the other part,

have agreed as follows:

**PROJECT Mosquito Control in Cross-border Area 2;**

**Ref. no. HR-RS253**

**CONTRACT TITLE Supply of vehicle with cold chamber for the project MOS-Cross2**

**Identification number HR-RS253-3/vehicle**

**Article 1 Subject**

* 1. The subject of the contract shall be the **supply** and **delivery** of the following supplies:

|  |  |  |
| --- | --- | --- |
| **Item no.** | **Product specification** | **Quantity** |
| 1 | **Vehicle with cold chamber** with next characteristics - **1 pc:**  - wheelbase (mm) – from 3100 to 3150  - vehicle length (mm) – from 4750 to 4850  - vehicle height (mm) – from 1850 to 1900  - vehicle width (mm) – from 1800 to 1850  - number of doors – 4 (four)  - number of seats – 2 (two)  - cargo space volume (m3) – from 4,1 to 4,4  - length of cargo space (mm) – from 2100 to 2200  - height of cargo space (mm) – from 1300 to 1350  - height of rear double doors (mm) – from 1240 to 1280  - side sliding door height (mm) – from 1150 to 1200  - weight of vehicle ready to drive (kg) – from 1450 to 1500  - load capacity of the vehicle ready to drive (kg) – from 900 to 940  - gross vehicle mass (kg) – from 2400 to 2450  Engine performance:  - number of cylinders – 4 (four)  - working volume (cm³) – from 1590 to 1600  - maximum power (kW / hp) at rpm – 88/120 at 3750  - Fuel – Eurodisel  - Exhaust emission standard – Euro 6d  - Gearbox type - manual 6 speed + R  - Gas tank – 60 liters  - Tires - 195/60 R16  Standard package with next items must be included:  - FPS fire protection system  - ABS + EBD (electronic brake force distribution)  - ESC (electrical stability control)  - Bluetooth + USB connects the radio of the device  - Power steering  - Metal partition wall of cargo space  - Electric windows  - Air conditioning  - Color: white  Vehicle must be isolated as follows:  The floor of the vehicle is paneled from waterproof plywood, insulation and covered with polyester with reinforcements due to the manipulation of loading goods. The floor thickness is 65mm. Thickness of thermally insulated sides 50 mm due to the required operating mode, all according to the declaration of the device manufacturer. All joints of the complete panels are filled with Sikaflex 521 UV sealant or equivalent so that the insulation composite closed. All built-in elements are certified for food transport. The insulation of the cargo space is adjusted to the technical construction of the vehicle, following the ratio of B and C pillars on the vehicle without disturbing the foundations of the factory elements of the structure.  Cold chamber must be adequate to operate in temperature mode + 2o C  Cold chamber system must be adequate for certification | 1 pc |

The place of acceptance of the supplies shall be **Novi Sad, Futoška no. 121** the time limits for delivery shall be **3 months** and the Incoterm applicable shall be **DDP**[[4]](#footnote-4) **excluding VAT**. The implementation period of tasks shall run from **November 10th 2021** to **February 10th 2022**.

1.2 The contractor shall comply strictly with the terms of the special conditions and the technical annex.

1.3 N/A.

**Article 2 Origin**

The rules of origin of the goods are defined in Article 10 of the special conditions.

A certificate of origin for the goods must be provided by the contractor at the latest when it requests provisional acceptance of the goods. Failure to comply with this condition may result in the termination of the contract and/or suspension of payment.

**Article 3 Price**

3.1 The price of the supplies shall be that shown on the financial offer (specimen in Annex IV). The total maximum contract price shall be <insert price> RSD.

3.2 Payments shall be made in accordance with the general and/or special conditions (Articles 26 to 28).

**Article 4 Order of precedence of contract documents**

The contract is made up of the following documents, in order of precedence:

* the contract agreement;
* the special conditions
* the general conditions (Annex I);
* the technical specifications (Annex II [including clarifications before the deadline for submission of tenders and minutes from the information meeting/site visit];
* the technical offer (Annex III [including clarifications from the tenderer provided during tender evaluation]);
* the budget breakdown (Annex IV);
* specified forms and other relevant documents (Annex V);

The various documents making up the contract shall be deemed to be mutually explanatory; in cases of ambiguity or divergence, they shall prevail in the order in which they appear above.

Done in English in three originals, two originals being for the Contracting Authority, and one original being for the Contractor.

|  |  |  |  |
| --- | --- | --- | --- |
| **For the Contractor** | | **For the Contracting Authority** | |
| Name: |  | Name: | **Prof. dr Vladimir Petrović** |
| Title: |  | Title: | **Acting Director** |
| Signature: |  | Signature: |  |
| Date: |  | Date: |  |

1. Where the contracting party is an individual. [↑](#footnote-ref-1)
2. Where applicable. For individuals, mention their ID card or passport or equivalent document – number. [↑](#footnote-ref-2)
3. Except where the contracting party is not VAT registered. [↑](#footnote-ref-3)
4. DDP (Delivered Duty Paid) - Incoterms 2010 International Chamber of Commerce - <http://www.iccwbo.org/incoterms/> [↑](#footnote-ref-4)