# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply and delivery of equipment for SARS-CoV-2 diagnostics for the project MOS-Cross2 p 1/2**

**Publication reference:** **HR-RS253-6/equipment for SARS-CoV-2 diagnostics**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | Multichannel (8-channel) electronic pipette, variable, volume 0,5-10 µl – 1 pc |  |  |  |
| **2** | Multichannel (8-channel) electronic pipette, variable, volume 10-100 µl – 1 pc |  |  |  |
| **3** | Mini centrifuge/vortex with rotor for 12 x 1,5/2 ml tubes and 2 x 8-section 0,2 ml microtube strips – 1 pc |  |  |  |
| **4** | Centrifuge for PCR plates 2 x standard (96 wells) plates – 1 pc |  |  |  |
| **5** | Single-channel pipette, variable, volume 0,5-10 µl – 1 pc |  |  |  |
| **6** | Single-channel pipette, variable, volume 10-100 µl – 1pc |  |  |  |
| **7** | Single-channel pipette, variable, volume 100-1000 µl – 1 pc |  |  |  |
|  | Delivery place must be Futoška no. 121, 21000 Novi Sad |  |  |  |
|  | Warranty period must be min. 2 (two) years from the date of provisional acceptance |  |  |  |